

Newland scanner OPOS setting

1, select NLScanner in device type



2, select HID-POS or COM based on customer’s demand, save



Newland OPOS scanner test

1, select NLScanner, open, claim, enable

